


**GAS 4 OPEN BURNER**

**900'**

**COOKING SERIE**





The stainless steel body makes the device durable and enduring.

Easy to clean through its rounded upper surface.

All burners are produced with special molds and pressed top.

The monoblock worktop increases the durability and ensures an easy cleaning.

In order to put pots pans etc on the stove burners, cast iron cooker burners are available.

Pilot flame taps with safety device have been used.


High efficiency and low gas emission burners have been used.

The thickness of the upper part is 1,5 mm AISI stainless steel.

The body sheets are 1 mm Scotch Brite stainless steel.

Can be used on countertop or on base cupboard.

Can be operated with LPG or natural gas.



G=GAS INLET

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **MODEL** | **DESCRIPTION** | **DIMENSIONS** | **TOTAL POWER** | **GAS CONSUMPTION** | | **WEIGHT** |
| GKO9020 | GAS BURNER | 800X900X280 | 40 kW | 4.233 max. / 2.222 min. | 3.155 max. /1.656 min. | 64 kg net |
| 820X960X450 Package dimension | G20(m3/h) | G30 (kg/h) | 74 kg Gross weight |



|  |  |  |  |
| --- | --- | --- | --- |
| **HEADQUARTER** | | **FACTORY** | |
| Plevne Caddesi No.40/C | | Taşpınar Mevkii No.154 | |
| Gülveren-Mamak/ANKARA | | Çubuk/ANKARA | |
| Tel . | +90 312 363 94 93 | Tel . | +90 312 837 76 72 |
| Fax. | +90 312 363 94 92 | Fax. | +90 312 837 73 38 |
| [**www.mutasgroup.com**](http://www.mutasgroup.com/) **/** [**info@vitalmutfak.com**](mailto:info@vitalmutfak.com) | | | |