


**GAS LAVASTONE GRILL**

**900'**

**COOKING SERIE**





All grills are designed for homogeneous temperature on the cooking surface.

Easy to clean through its rounded upper surface.

The device is produced with special molds and pressed top.

The stainless steel body makes the device durable and enduring.

The specially designed cast gril makes the waste oil accumulating on the discharge at the front.

Adjustable cooking surface temperature.

Safety gas valves provide safe operation.

A thermocouple for flame control is available.

Has a piezoelectric ignition system.


The waste oil is collected on the removable container which makes it easy to clean.

The thickness of the upper part is 1,5 mm AISI stainless steel.

The body sheets are 1 mm Scotch Brite stainless steel.

Can be used on countertop or on base cupboard.

Can be operated with LPG or natural gas.



G=GAS INLET

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **MODEL** | **DESCRIPTION** | **DIMENSIONS** | **TOTAL POWER** | **GAS CONSUMPTION** | | **WEIGHT** |
| GLI9020 | GAS LAVASTONE GRILL | 800X900X280 | 19 kW | 2.011 max. / 1.056 min. | 1.498 max. /0.787 min. | 123 kg net |
| 820X960X530 Package dimension | G20(m3/h) | G30 (kg/h) | 133 kg Gross weight |



|  |  |  |  |
| --- | --- | --- | --- |
| **HEADQUARTER** | | **FACTORY** | |
| Plevne Caddesi No.40/C | | Taşpınar Mevkii No.154 | |
| Gülveren-Mamak/ANKARA | | Çubuk/ANKARA | |
| Tel . | +90 312 363 94 93 | Tel . | +90 312 837 76 72 |
| Fax. | +90 312 363 94 92 | Fax. | +90 312 837 73 38 |
| [**www.mutasgroup.com**](http://www.mutasgroup.com/) **/** [**info@vitalmutfak.com**](mailto:info@vitalmutfak.com) | | | |